Type:

Data packet 00

Control packet

PE

Input Number and Bias 01

Weight 10

Switch

Forwarding table 11

Data Packet

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 2 | 5 | 8 | 8 | 10 |
| type | sequence number | index | source | input |

Input Number & Bias

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 2 | 5 | 8 | 8 | 10 |
| type | sequence number | destination | input number | bias |

Weight

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 2 | 5 | 8 | 8 | 10 |
| type | sequence number | destination | source (weight) | weight |

Forwarding table

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 2 | 8 | 4 | 3 | 16 |
| type | row number | fractional  number | optional | data |